DSCP

A Differentiated Services Code Point (DSCP) is a 6-bit code point in the differentiated services field (DS field) inside the packet IP header.

It is used by Differentiated Services for classification purposes to provide quality of service functionality.