Flow Control

Ethernet flow control is a mechanism for temporarily stopping the transmission of data on Ethernet family computer networks.

The goal is to regulate traffic in order to prevent packet dropping.