QoS Mark

The Quality of Service Mark is used when classifying traffic. Packets matching the filter will be marked with the provided hexadecimal code 0x000000-0xFFFFFF.

This mark can then be used for identification and filtering purposes, for example by iptables .